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ABSTRACT

This research is reporting of the skid adjustment method of the dynamically by using active brake force control to improve vehicle stability in various driving condition Electric Vehicle passenger car. The presence of skid is determined by comparing the tires rotational speed and the free-rolling speed. A two wheels front steering 2 Wheel Steer system Electric Vehicle are used in this work. Discrepancy of the measured velocities between these sensors indicates the presence of skidding. When the Electric Vehicle performing a turning motion, the measured yaw rates from both sensors with a steering angle sensor added can also be used and compared to observe the skidding that indicates either understeer or oversteer. Ackerman calculation are used to investigate the motion of the 2 Wheel Steer  Electric Vehicle respectively. Compensated moment for this research is use for braking system, such as acceleration, braking, when turning or straight, and Fuzzy logic as controlling system using Simulink Matlab as its simulator. The results of this simulation will be analyzed can compare to show the improved performance.
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NOMENCLATURE
EV	Electric Vehicle
ESC	Electronic Stability Control
	Vehicle moment
	Acceleration [m/sec2]
	Vehicle mass [kg]
	Gravity acceleration [m/sec2]
	Vehicle speed [km/hr]
	Start Vehicle speed [km/hr]
	Ackerman / ideal turn radius [m]
	Angle steer front wheel [rad.]
	Side-slip angle [rad.]
	Slip angle front wheel [rad]
	Slip angle rear wheel [rad]
	Braking force [N]
	Centrifugal force[N]
	Cornering force[N]
	All lateral force [N]
	Vehicle weigh [N]
	Normal force[N]
	Friction wheel longitudinal
	Friction Wheel lateral
	Yaw rate Ackerman [rad/sec]
	Yaw rate response [rad/sec]

1.0  INTRODUCTION
In a passenger car, the safety of the passenger is the main priority. From the engineering perspective, the passenger’s safety is closely related to the vehicle stability by ensuring the ability to maneuver under extreme drive conditions such as sudden braking, high acceleration, sudden turning to avoid obstacles and turning at a high speed[1]. The extreme driving gives rise to unstable vehicle conditions which are very dangerous. The vehicle stability might be attained back by compensating the forces and moments which brought the vehicle to unstable through a wheels traction control and braking[2].   Figure 1 shows slip caused events that can happen to vehicles with lacking an adequate stability system during high-speed maneuver. 
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Figure 1. Condition Vehicle

Wheel slip arises when a particular wheel fails to withstand forces larger than its friction force between the wheel and road surfaces. Under this condition, the vehicle is difficult to be controlled by an ordinary driver and it can be considered that the vehicle is losing its stability. This vehicle slip may include events of oversteer or understeer that could jeopardize the safety of the passengers.

Electronic stability control (ESC) technology has been applied to fuel combustion passenger car. Application of the technology was done by the leading automobiles manufacturers such as BMW, Mercedes, Volvo and etc. The technology had already applied in developed countries that all the cars have to have an ESC installed to reduce the road car accidents[3]. Regulation of ESC technology application in Europe had been done since 2014 for all cars and the latest productions[3].

ESC includes sensors such as wheel speed sensor, yaw rate sensor, a lateral acceleration sensor, and steering wheel sensor to identify the dynamics of the vehicle[1]. ESC has the different mode of yaw stability control and roll stability control. In this study, yaw stability control mode is discussed. In yaw stability control mode, the ESC calculates[2]:

· Heading of the vehicle using steering angle sensor and vehicle speed sensor.
· The Radius of the current path using lateral acceleration sensor and vehicle speed.
· Correct yaw rate of the vehicle traveling on the path by calculated radius and measured vehicle speed using onboard yaw rate sensor from which ESC system measures actual yaw rate.

In an ESC system usually, a microcontroller based system does the calculations mentioned above and estimates the intended heading and ideal motion then compares them with the actual motion[4]. If the difference between the measured yaw rate and calculated yaw rate exceeds the threshold value then the ESC system sends control signals to the actuators to apply corrective forces on the vehicle. There are a number of different techniques for correcting the vehicle motion. ESC in the conventional vehicles with single electric motor has limitations for control with the existing resources, so different additional sensors and actuators are introduced in different techniques of ESC. Providing the expected longitudinal response the driver needs is another key point to focus on for ESC. In this research different types of ESC are briefly discussed and analyzed to find a suitable type for the proposed Electric Vehicle. Then an ESC is proposed with ABS braking and Fuzzy logic. Controller. Fuzzy logic controller is used for set distribution ABS braking, when the electric vehicle acceleration and turn. So, the controller can set the braking for each wheel. 

2.0 VEHICLE DYNAMIC
Though different methods of finding wheel torque are adopted in different research for ESC, the vehicle model is similar in most of the research works. Difference can be seen in the degree of freedom of the vehicle model. The vehicle model is required for the simulation to observe the responses of the vehicle body. This vehicle body model can then be used as a plant vehicle. In other research work a vehicle model is employed for a four-wheel-drive electric vehicle with the equation of motion of vehicle dynamics[1]. Equation of motion when the vehicle having plane motion is given here
                	(1)     
 	(2)
 		(3)
Where,  is longitudinal velocity of the vehicle,  and  denote side slip and yaw rate.
  			(4)

2.1 Turning Vehicle Dynamic
Turning on vehicle will happen when input from steering, this condition must be response fast with Electronic Control Unit (ECU). When the ECU detect oversteer, oversteer this vehicle doing brake for rear right wheel and understeer condition oversteer this vehicle doing brake for rear right wheel, when under steer brake rear left wheel with make proportion brake when turning[1,2]. Vehicle condition when turning can see at figure 2. 
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Figure 2. Force and Moment on Vehicle When turning

Analysis of normal force on each wheel on sloping and incline road conditions can be formulated as follows :
· Front Left  Wheel
 (5)
· Rear Left Wheel
 (6)

· Front Right Wheel
 (7)

· Rear Right Wheel
 (8)

2.2 Force Braking
According The national high traffic safety administration, Force braking is the emergency condition braking system caused the vehicle to stop. The braking force on each wheel can be shown as follow:
					  (9)
· Straight – down
 
  	 (10)
· Turning – down
 
 (11)
where,
 					  (12)
Force  works on tires contact with the opposite direction of (Fx) and has magnitude as . Maximum allowable braking force occurs in adhesive maximum limit tire-road tires on the structure when slip angle of 40 and the percentage of skid 20% on the normal force, resulting in the maximum Automatic Braking System (ABS) braking can be formulated for each tire[6-7]. The proportion of Automatic Braking System(ABS) braking for each tire is the ratio between the maximum brake force of the tire to the total braking force of all wheels,
 
  					  (13)
The proportion of Automatic Braking System (ABS) braking of each tire is the ratio between the maximum brake force of the tire to the total braking force of all wheels:
 				  (14)
where,
   				  (15)

2.3 Setting Force Braking by ABS
Critical deceleration during braking which resulted in longitudinal skid obtained as follow:
· Straight /down
 	  (16)
 
· Turning /down
 					  (17)

From equations 16 & 17 by eliminating Ra and Rr, resulting in a critical deceleration rate each tire is used as setting deceleration:
· Straight /down
 		  (18)
· Turning/down
  	  (19)

In this way we can determine the order of occurrence of lock tendencies (resulting in longitudinal skid above 20%) on all four wheels, small deceleration rate goes first lock on . ABS controls the proportion of braking of each wheel according to its deceleration rate[7].

2.4 Centrifugal Force and Wheel Slip Angle
Centrifugal force is divided into the front and rear wheels lead to slip angle as follows:
· Front wheel
 				  (20)
· Rear wheel
  				  (21)
Where,
 
 
Distribution of static condition weight on front wheel and rear wheel[9],
 					  (22)
 					  (23)
Then,
 				  (24)
 				  (25)
Slip angle at front wheel and rear wheel,
 
      				  (26)
 
 				  (27)
when,
 				  (28)
so,
  			  (29)

2.5 Characteristics of Adhesion between Road and Tire
The friction force is caused by the slip that occurs between the drive wheel and the road surface. During the acceleration causing the slip (λ) on the wheels[9], it is formulated by the following equation:
 				  	  (30)
where,
V = Vehicle speed (km/h)
r = Radius(m)
 = Angle wheel speed (rad/s)
In the seventies, some researchers including Easton, Moore, Taborek[8] proposed a concept of tire and road contacts that altered an existing braking and concerning effort concept. The principle of the ABS system concept is to keep the wheel slip (λ) as expected (desired range), so that the optimum braking condition is obtained.

2.6 Yaw rate
The yawing rate is the moment of inertia to the axis Z arises at the center of mass. The yaw rate can be distinguished either by a steady state yaw rate or dynamic yaw rate condition. In a condition where the moment of inertia of the vehicle is absent, the turn state by assuming angle parameter of steer (δ), turning radius (R) and vehicle velocity (V) constant[9].  Steady-state yaw rate determination for 2WS vehicle used standard Ackerman: 
 				 	  (31)
Given the effect of the slip angle to yaw rate, actual gain becomes, 
 
          			  (32) 
From the above equation, it can be seen that it affects the turning properties Kus(turn coeficien). If the Kus < 0 the vehicle will undergo oversteer, and if Kus > 0 understeer happens whilst if Kus = 0  normal or neutral behavior takes place. So to make a neutral turn it needs to be controlled so that  and  can be the same. This is done by reducing the proportion of the application of braking forces to control the slip percentage (λ). Yaw rate condition using for detect vehicle when turning, it can detect understeer and over steer. This is the actual heading for vehicle. 

2.7 Dynamic Condition
Yaw rate dynamic occurs due to the acceleration of yaw steady in the form of acceleration yawing, due to changes in input angle steer (δ).
The actual yawing of the vehicle dynamic conditions is formulated as follows, 
 	  (33)
Acceleration of yawing under steady state 
 
 	  (34)
The yawing acceleration occurring as a result of the skidding motion is shown as 
 	(35)
where,
 
 
with,
  	
  
 
 	(36)
direction to turn according to Ackerman then, 
 	(37)
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Figure 3. Flowchart Calculation Algorithm

3.0  ALGORITHM 
The calculation method used is quasi-dynamic quantification method where the dynamic condition of the vehicle is analyzed partly as if in a static condition and then used the simulator to get the simulation result with high time increment resolution/density with numerical calculation effort mostly done by computer. The calculation algorithm is shown in Figure 3. Model for this vehicle is use Simulink Matlab. The first input parameter for Ackerman condition, Force moment, inertia moment, and tire moment, and then can analysis of  skid with fuzzy logic use Simulink Matlab[11]. Next step is analysis vehicle motion with skid and get real motion vehicle. 
 

3.1 Calculation algorithm
The results of this simulation are still limited in numerical form and in the form of plot diagrams. have not produced a form graphical.

3.2 Brake force controller
Brake force FB for each wheel is adjusted by considering the slip requirement, which is obtained from Fuzzy Logic Controller output. So Active Brake Force Control is obtained by altering the slip setpoint dynamically based on Yaw Rate Real Response ratio of the vehicle with Yaw Rate Neutral. Figure 4 explain how the work of Brake Force Controller.
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Figure 4. Brake force Controller

3.3 Fuzzy Logic Controller for ESP
By using Mamdani method on Fuzzy Logic Controller, and with the condition Member Function and Rule used is good enough it will get the result of controlling responsive that does not happen overshoot which is too big and optimal enough[12,15] so not too burdening resources from controller engine. For this controller use two input yaw are netral and response, and have two output for right wheel and left wheel. It can see at figure 5. For this experiment have 17 Rule. 
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Figure 5. Fuzzy Logic Controller For ESC

With the ability to control the braking force against all four wheels of the vehicle, during cruise, deceleration and acceleration at various steer angles and road and surface conditions, the forces that generate an unsuitable Yaw Rate will be overcome by providing a force on the brakes of each wheel which requires a variety of driving conditions.

4.0 SIMULATION RESULT
Using the calculation method and simulator as described, we have generated numerical data from the simulation by applying controlled parameters on ESP model. The lack of accuracy of the simulation results from Simulink Matlab is due to the following described limitation:

* Vehicle direct braking from initial velocity V0 from initial time t0, so there is no comparison between steady-state (for example during cruise without interruption) and transient conditions (beginning to end braking).

* Vehicle brakes while turn, where the turning is given in the form of step signal whose value changes one time during braking takes place→ there is two value steer angle in one braking ( one value discontinuous, two the same value with opposite direction).

* Yaw responses and slip responses are obtained based on calculations, later on, real conditions use gyro sensors and speed sensors on each wheel.

* The representation of left and right wheel subscript here is meant, the left wheel represents the forces or moments that the vehicle rotates to the left at yaw axis, and the right wheel also.

The simulation test uses the steer angle conditions. It appears that the steer angle as a step function with a value of 5̊ at t = 0 and -5̊ at t = 1 sec with initial velocity V0 = 200 {km/h} and at the moment when t = 0 in which the braking has been started.

In Figure 6, the proportion of left and right wheel brake force, it appears when t = 1 second, the right wheel braking force rises drastically and the left wheel braking force drops dramatically, this is due to a steering angle where the steer angle position of the + 5 ̊ is rapidly changed to the -5̊  and at t ≈ 2 the braking force of the two wheels approach almost the same value, due to the condition being closed to the steady state.
[image: ]
Figure 6. Proportion braking force at Right wheel and left wheel

Figure 7 shows the output of the fuzzy logic controller, which is used as the input set point of the ABS controller. It appears that the setpoint of ABS is a dynamic function of the vehicle's directional behavior, not static at only 0.2.

The moment that works on the vehicle body on the yaw axis can be seen in Figure 8, where it appears that there is a very large moment change in the event of steer angle change, and in relatively short period of time, the system is returned to steady-state conditions (not fully ideal) by the work of the controller. Proportion brake on right wheel and left wheel is different.
[image: ]
Figure 7. Setpoint slip output from fuzzy logic controller

[image: ]

Figure 8. Total moment on yaw (Z)

[image: ]
Figure 9. Yaw response and Ackerman

Figure 9. can be explain that condition slip at electric vehicle. Yaw rate response can follow yaw rate Ackerman’s path. But, at 10 seconds the vehicle detects overshoot when the vehicle is turning, so this condition named oversteer. When vehicle detects oversteer, it must be keep up on the track.

5.0 CONCLUSION
This paper presented the use Electronic Stability Control for the Electric vehicle. With the active brake force control, the control of vehicle stability can be improved, So the use of ESP Controller can improve the ability to control the stability of vehicle. This Condition used for compensated yaw moment for an electric vehicle. Compensated moment use right wheel and left wheel when turning. 
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